
[-defdefine LessonName "Adding a New Runup Pad"-]
<section id='BaseOps_Tutorial_AddingRunupPad_id'>
    [-include "BaseOps_SetUpStandardWorkbookCase.tutscript"-]
    <title>
        &LessonName;
    </title>
    <section>
        <title>
            &LessonName;
        </title>
        <para>
            This tutorial series assume that you are a base planner with limited
            noise modeling experience. Any major editing of your installation's
            BaseOps case will likely be done by a third party. However, it
            is hoped that this tutorial series will give you the necessary
            skills to make minor changes yourself.
        </para>
        <para>
            One such minor change is adding a new static pad and setting the
            runup operations that occur there. This lesson will teach you
            how to do this. It is presented as a list of step-by-step instructions.
            To begin, press the <bold>First Step</bold> button below.
        </para>
    </section>
    <section>
        <title>
            Step 1
        </title>
        <para>
            Go to the object type selector dropdown list in the upper-left
            corner of the BaseOps window, and select "Static Pads".
        </para>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 1.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 2
        </title>
        <para>
            Add a new static pad. To do this, first activate the Add mouse
            tool by pressing its button <img
            src='intres:BaseOps_AddTool_ToolbarButton'/> on the toolbar. Then,
            click on the location where the static pad is located.
        </para>
        <note type='tip'>
            <para>
                If may be useful to zoom the map in on the location where you
                will be adding the new pad.
            </para>
        </note>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 2.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 3
        </title>
        <para>
            Give your new static pad a descriptive name. First click on the
            box labeled Name, then type the new name.
        </para>
        <note type='note'>
            <para>
                The new name must be 10 characters or less.
            </para>
        </note>
        <note type='tip'>
            <para>
                You may want to set the new pad's Long Name field to a longer,
                more descriptive name. Also, it is suggested that you use the
                Notes field to record any miscellaneous notes about this new pad.
            </para>
        </note>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 3.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 4
        </title>
        <para>
            Now we will set the operations that occur at this pad. Go to the
            object type selector dropdown list in the upper-left corner of
            the BaseOps window, and select "Static Profiles".
        </para>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 4.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 5
        </title>
        <para>
            A static profile is a record of the runup operations that an aircraft
            performs at a static pad. You will need to add one static profile
            for each combination of aircraft, engine, and noise suppressor
            that is used at the pad.
        </para>
        <para>
            Add the first static profile by pressing the Add Static Profile
            button <img src='intres:WCF_AddPlusSignToolbarButtonBitmap'/>,
            located above the list on the left side of the BaseOps window.
        </para>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 5.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 6
        </title>
        <para>
            Set the name of the new static profile.
        </para>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 6.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 7
        </title>
        <para>
            Go to the dropdown list labeled Pad, and select the new static
            pad you just added.
        </para>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 7.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 8
        </title>
        <para>
            In the box labeled Heading, type the magnetic heading of the aircraft
            when performing runups on this pad. This is the direction the
            plane's nose is pointing, measure in degrees clockwise from magnetic
            north.
        </para>
        <note type='note'>
            <para>
                If the aircraft performs static runups while pointed in two or
                more directions, separate static profiles must be created for
                each direction.
            </para>
        </note>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 8.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 9
        </title>
        <para>
            In the dropdown list labeled Aircraft, select the aircraft operating
            on this pad. Then, in the next two dropdown lists, select the
            aircraft engine and the noise suppression method used.
        </para>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 9.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 10
        </title>
        <para>
            In the dropdown list labeled Power Units, select the engine power
            units used to express the aircraft's power settings.
        </para>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 10.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 11
        </title>
        <para>
            Aircraft runup operations are expressed in terms of segments.
            Each segment models the running of one or more aircraft engines
            for a specific power setting and duration. An example of a segment
            is running an F-16 at 70 % RPM idle power for 300 seconds.
        </para>
        <para>
            Decide how many segments you will need to model your aircraft's
            static operations, then press the Add New Segment button <img
            src='intres:WCF_AddPlusSignToolbarButtonBitmap'/> , located in
            the lower-right portion of the BaseOps window, to add the segments.
            The segments will be added to the segment table.
        </para>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 11.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 12
        </title>
        <para>
            In the Power column of the segment table, type the numeric power
            level, then choose the operation power description (for example,
            "Idle").
        </para>
        <note type='note'>
            <para>
                For some operation power descriptions (for example, "Max A/B"),
                the numeric power level is fixed and cannot be changed.
            </para>
        </note>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 12.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 13
        </title>
        <para>
            In the Day Ops, Evening Ops (if applicable), and Night Ops columns
            of the segment table, enter the average number of times per day
            that this segment is performed during each of these periods.
        </para>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 13.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 14
        </title>
        <para>
            In the Duration column of the segment table, enter the length
            of time that the aircraft engines are run for each of the segments.
        </para>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 14.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 15
        </title>
        <para>
            In the Num Engines column of the segment table, enter the number
            of engines that are simultaneously run as part of this segment.
        </para>
        <para>
            [-include "BaseOps_ShowMeHowLink.rxl" VideoName='BaseOps_AddingRunupPad - 15.wcsaf'-]
        </para>
    </section>
    <section>
        <title>
            Step 16
        </title>
        <para>
            Repeat steps 4-15 to add any additional static profiles. Once
            they have been added, you can run the case and view the new noise
            contours. Running the case and viewing the noise contours are
            covered by other lessons in this tutorial series.
        </para>
    </section>
</section>
